NOTE:  The WVACO5.PFL file contains the on-site data for input to AERMET.  These data were
constructed from the 100m Met tower located on a ridge about 900m east-southeast of the 
facility and the 30m Luke Hill tower located on a ridge about 900m north-northwest of the 
facility.  The 210m level (above stack base) is based on the 30m level (above local ground) 
of the  Luke Hill tower.  Since AERMET requires the reference wind measurement to be below 
100m, the 210m level wind data were duplicated as 30m data for use as the reference wind 
by AERMET.  The WVACO4.PFL file contains the 4-level profile file for input to AERMOD, in 
which the 30m level has been removed in order to avoid its use in generation of vertical 
wind profiles within AERMOD.  The WVACO4.PFL file contains the same 4-level profile data 
used in the evaluation of CTDMPLUS on the Westvaco dataset.

RWB