# Control packet for Regional Haze BART determinations
# Provided by Martha Keeting (AQPD-EPA) 12/3/2013
# Made the effective date 1/1/2018 for all controls
# For analysis, see spreadsheet:
#   /garnet/oaqps/em_v6/2011platform/work/projections/Non_EGU_Inventory_updates_Regional_Haze_2018_11_18_13_AZ.xlsx
#fips,scc,poll,pri_CM_abbrev,ceff,reff,rpen,sic,mact,application_control,replacement,plantid,pointid,stackid,segment,compliance_date,NAICS,comments
#EXPORT_DATE=Fri Nov 21 14:35:50 EST 2014
#EXPORT_VERSION_NAME=Initial Version
#EXPORT_VERSION_NUMBER=0
13051;;"SO2";;47.25027274;100.0;100.0;;;Y;A;"3679811";;;;2018-01-01 00:00:00;! International Paper - Savannah Containerboard Mill, ceff calculated based on total facility SO2 reduction of 2000 tons
13099;;"SO2";;70.0;100.0;100.0;;;Y;A;"931711";;;;2018-01-01 00:00:00;!  Georgia Pacific - Cedar Springs
13127;;"SO2";;58.62513637;100.0;100.0;;;Y;A;"3721011";;;;2018-01-01 00:00:00;! Georgia Pacific - Brunswick.  Emission reductions greater than total emissions, so averaged the % reduction from 2 similar facilities in GA: Georgia Pacific Cedar Springs and International Paper Savannah
16027;;"SO2";;65.0;100.0;100.0;;;Y;A;"931611";;;;2018-01-01 00:00:00;!  The Amalgamated Sugar Company (Tasco)
16027;;"NOX";;80.0;100.0;100.0;;;Y;A;"931611";;;;2018-01-01 00:00:00;!  The Amalgamated Sugar Company (Tasco)
26029;;"NOX";;50.0;100.0;100.0;;;Y;A;"8160611";;;;2018-01-01 00:00:00;! St. Mary's Cement-Charlevoix
26103;;"SO2";;86.89775031;100.0;100.0;;;Y;A;"8062611";"7179413";;;2018-01-01 00:00:00;! Tilden. Summed two largest kilns and calculated ceff from combined  emission reduction of 3230 tons NOx and 900 tons SO2
26103;;"NOX";;60.57764441;100.0;100.0;;;Y;A;"8062611";"7179413";;;2018-01-01 00:00:00;! Tilden. Summed two largest kilns and calculated ceff from combined  emission reduction of 3230 tons NOx and 900 tons SO2
26103;;"SO2";;86.89775031;100.0;100.0;;;Y;A;"8062611";"7178813";;;2018-01-01 00:00:00;! Tilden. Summed two largest kilns and calculated ceff from combined  emission reduction of 3230 tons NOx and 900 tons SO2
26103;;"NOX";;60.57764441;100.0;100.0;;;Y;A;"8062611";"7178813";;;2018-01-01 00:00:00;! Tilden. Summed two largest kilns and calculated ceff from combined  emission reduction of 3230 tons NOx and 900 tons SO2
27137;;"NOX";;85.37824024;100.0;100.0;;;Y;A;"6237711";;;;2018-01-01 00:00:00;! Arcelor Mittal. Used facility total emissions to calculate ceff for 2859 tons NOx reduction
27137;;"NOX";;90.02062413;100.0;100.0;;;Y;A;"6237611";;;;2018-01-01 00:00:00;! Hibbing Taconite.  Emission reductions greater than total emissions, so averaged the % reduction from 2 similar facilities: Arcelor and US Steel Minntac
27075;;"NOX";;90.02062413;100.0;100.0;;;Y;A;"6319411";"16394813";;;2018-01-01 00:00:00;! Northshore Mining, furnace specific emissions.  Emission reductions greater than total emissions, so averaged the % reduction from 2 similar facilitiesr, Arcelor and US Steel Minntac
27075;;"NOX";;90.02062413;100.0;100.0;;;Y;A;"6319411";"16396413";;;2018-01-01 00:00:00;! Northshore Mining, furnace specific emissions.  Emission reductions greater than total emissions, so averaged the % reduction from 2 similar facilities, Arcelor and US Steel Minntac
27137;;"SO2";;90.0;100.0;100.0;;;Y;A;"6239611";;;;2018-01-01 00:00:00;! United Taconite. For NOx, using facility wide emissions to calulculate ceff for a reductioni of 3208 tons.  For SO2, emission reductions greater than total emissions; therefore using CoST control measure SFGDSMIPR ceff (effective date 1/2020)
27137;;"NOX";;73.6655372;100.0;100.0;;;Y;A;"6239611";;;;2018-01-01 00:00:00;! United Taconite. For NOx, using facility wide emissions to calulculate ceff for a reductioni of 3208 tons.  For SO2, emission reductions greater than total emissions; therefore using CoST control measure SFGDSMIPR ceff (effective date 1/2020)
27061;;"NOX";;92.29694988;100.0;100.0;;;Y;A;"13598411";;;;2018-01-01 00:00:00;! US Steel Keetac. Calculated facility wide ceff for NOx reduction of 2908 tons.
27137;;"NOX";;94.66300803;100.0;100.0;;;Y;A;"6927911";;;;2018-01-01 00:00:00;! US Steel Minntac. Calculated facility wide ceff for NOx reduction of 6077 tons.
30043;;"NOX";;76.39996082;100.0;100.0;;;Y;A;"7766911";;;;2018-01-01 00:00:00;! Ash Grove Cement. Calculated facility wide ceff for NOx reductions of 1088 tons
36113;;"NOX";;50.0;100.0;100.0;;;Y;A;"8325311";"133713";;;2018-01-01 00:00:00;! Lehigh Northeast Cement, kiln specific
39141;;"SO2";;76.58079143;100.0;100.0;;;Y;A;"8131111";"6005113";;;2018-01-01 00:00:00;! P. H. Glatfelter Company - Chillicothe, Boiler #7. Summed emissions across boiler #7 and #8 and calculated ceff for combined SO2 reduction of 4550 tons
39141;;"SO2";;76.58079143;100.0;100.0;;;Y;A;"8131111";"6003213";;;2018-01-01 00:00:00;! P. H. Glatfelter Company - Chillicothe, Boiler #8. Summed emissions across boiler #7 and #8 and calculated ceff for combined SO2 reduction of 4550 tons
47163;;"SO2";;90.0;100.0;100.0;;;Y;A;"3982311";;;;2018-01-01 00:00:00;! Eastman Chemical company
51580;;"SO2";;15.0;100.0;100.0;;;Y;A;"5798711";;;;2018-01-01 00:00:00;! Meadwestvaco Packaging plant - Covington. Emissions were tiny for the activated carbon facility, so applying to the packaging plant.
55009;;"SO2";;86.4106623;100.0;100.0;;;Y;A;"4943811";;;;2018-01-01 00:00:00;! Georgia pacific had two facilities very close to each other.  Combined emissions across facilities and calculted ceff for NOx cap of 1297 tons and SO2 cap of 1700 tons.
55009;;"NOX";;63.36320263;100.0;100.0;;;Y;A;"4943811";;;;2018-01-01 00:00:00;! Georgia pacific had two facilities very close to each other.  Combined emissions across facilities and calculted ceff for NOx cap of 1297 tons and SO2 cap of 1700 tons.
55009;;"SO2";;86.4106623;100.0;100.0;;;Y;A;"4944011";;;;2018-01-01 00:00:00;! Georgia pacific had two facilities very close to each other.  Combined emissions across facilities and calculted ceff for NOx cap of 1297 tons and SO2 cap of 1700 tons.
55009;;"NOX";;63.36320263;100.0;100.0;;;Y;A;"4944011";;;;2018-01-01 00:00:00;! Georgia pacific had two facilities very close to each other.  Combined emissions across facilities and calculted ceff for NOx cap of 1297 tons and SO2 cap of 1700 tons.
/END/
