/PROJECTION 2011 2018/
# packet for 2011v6 platform
# Additional CONTROL packet from emission decreases/closures or otherwise chosen not to be included here
# Impacts ptnonipm sector only
# From comments by AL, VA, ME and TCEQ
# Maine: 09sep13, 9:53pm from Karla Buchanan [Karla.Buchanan@maine.gov]: NonEGU_Point_Nonpoint_Projections_Data_KHB.xlsx
# VA: 18 and 22jul13 thread from Doris McLeod (DEQ) [Doris.McLeod@deq.virginia.gov]:VA_DEQ_nonEGU_controls-NOx and NH3 reductions.xlsx
# ...plus numerous Enclosure [I-IV.pdf] files
# TCEQ: 31may13 and 27aug13 data from Kevin Cauble: [kevin.cauble@tceq.texas.gov]
# AL: 3dec13 from Anna Watkins: Edited AL EPA 2011 pointsource_rm.xlsx
# Reconcile cement plant from ISIS packet, remove 2 units that close: FIPS=48139, FACILITY_ID=4852711, unit_ids: 31647413, 31647513
# Also reconcile ISIS cement to remove NOX and PM only for: FIPS=01091, FACILITY_ID=1002911, unit_id: 91072713
# THIS PACKET EXPORTED FROM: /garnet/home/rhc/2011v6/mk_CONTROL_PP_state_comments.sas
#EXPORT_DATE=Tue Aug 23 12:19:45 EDT 2016
#EXPORT_VERSION_NAME=Initial Version
#EXPORT_VERSION_NUMBER=0
"01053";;1.076798246;"CO";;;"985111";"47832513";"45375512";"47832513";;! From AL DEM Anna Watkins: Escambia Operating Company LLC
"01053";;1.076897568;"NOX";;;"985111";"47832513";"45375512";"47832513";;! From AL DEM Anna Watkins: Escambia Operating Company LLC
"01053";;0.928162481;"PM10-PRI";;;"985111";"47832513";"45375512";"47832513";;! From AL DEM Anna Watkins: Escambia Operating Company LLC
"01053";;1.629613325;"PM25-PRI";;;"985111";"47832513";"45375512";"47832513";;! From AL DEM Anna Watkins: Escambia Operating Company LLC
"01053";;0.616590707;"SO2";;;"985111";"47832513";"45375512";"47832513";;! From AL DEM Anna Watkins: Escambia Operating Company LLC
"01091";;1.120781128;"NOX";;;"1002911";"91072713";"45288912";"123538214";;! From AL DEM Anna Watkins: CEMEX Inc
"01091";;0.808366361;"PM10-PRI";;;"1002911";"91072713";"45288912";"123538214";;! From AL DEM Anna Watkins: CEMEX Inc
"01091";;0.808366361;"PM25-PRI";;;"1002911";"91072713";"45288912";"123538214";;! From AL DEM Anna Watkins: CEMEX Inc
"01091";;1.120781128;"NOX";;;"1002911";"91072713";"45290612";"123538114";;! From AL DEM Anna Watkins: CEMEX Inc
"01091";;0.808366361;"PM10-PRI";;;"1002911";"91072713";"45290612";"123538114";;! From AL DEM Anna Watkins: CEMEX Inc
"01091";;0.808366361;"PM25-PRI";;;"1002911";"91072713";"45290612";"123538114";;! From AL DEM Anna Watkins: CEMEX Inc
"01131";;1.048423789;"NOX";;;"10633711";"58474313";"54229512";"76744414";;! From AL DEM Anna Watkins: International Paper
"01131";;0.382882883;"SO2";;;"10633711";"58474313";"54229512";"76744414";;! From AL DEM Anna Watkins: International Paper
"01131";;0.969592761;"NOX";;;"10633711";"58474513";"54229712";"76744514";;! From AL DEM Anna Watkins: International Paper
"01131";;1.011033337;"SO2";;;"10633711";"58474513";"54229712";"76744514";;! From AL DEM Anna Watkins: International Paper
"01131";;0.969565643;"NOX";;;"10633711";"58474613";"54229712";"76744614";;! From AL DEM Anna Watkins: International Paper
"01131";;1.011033337;"SO2";;;"10633711";"58474613";"54229712";"76744614";;! From AL DEM Anna Watkins: International Paper
"01131";;1.012012012;"SO2";;;"10633711";"58474713";"54229612";"76744714";;! From AL DEM Anna Watkins: International Paper
"01131";;0.969579532;"NOX";;;"10633711";"58474813";"54229712";"76744814";;! From AL DEM Anna Watkins: International Paper
"01131";;1.011033337;"SO2";;;"10633711";"58474813";"54229712";"76744814";;! From AL DEM Anna Watkins: International Paper
"01131";;1.021220159;"NOX";;;"10633711";"83314813";"74527012";"108493914";;! From AL DEM Anna Watkins: International Paper
"01131";;1.021212121;"SO2";;;"10633711";"83314813";"74527012";"108493914";;! From AL DEM Anna Watkins: International Paper
"23005";;2.1127;"SO2";;;"5823511";;;;;! FPL ENERGY WYMAN LLC
"23011";;2.2059;"NOX";;;"5691611";;;;;! HUHTAMAKI INC - WATERVILLE
"23013";;1.4535;"NOX";;;"5692011";;;;;! FMC BIOPOLYMER
"23025";;9.2593;"NOX";;;"5253911";;;;;! project at facility-level, switching to natural gas: MADISON PAPER INDUSTRIES
"48139";;5.75;"106990";;;"4852711";"31648813";"30263612";"10479314";;! Cement Kiln Changes: Future emissions are based on permit 1 maximum allowable emission rates.  Wet kiln will be reconstructed to a preheater/precalciner. Ash Grove will use good combustion practices as BACT for VOC (0.138 lb/ton clinker, 12-month rolling period) for the kiln system.: Ash Grove
"48139";;5.75;"107028";;;"4852711";"31648813";"30263612";"10479314";;! Cement Kiln Changes: Future emissions are based on permit 1 maximum allowable emission rates.  Wet kiln will be reconstructed to a preheater/precalciner. Ash Grove will use good combustion practices as BACT for VOC (0.138 lb/ton clinker, 12-month rolling period) for the kiln system.: Ash Grove
"48139";;5.75;"50000";;;"4852711";"31648813";"30263612";"10479314";;! Cement Kiln Changes: Future emissions are based on permit 1 maximum allowable emission rates.  Wet kiln will be reconstructed to a preheater/precalciner. Ash Grove will use good combustion practices as BACT for VOC (0.138 lb/ton clinker, 12-month rolling period) for the kiln system.: Ash Grove
"48139";;5.75;"67561";;;"4852711";"31648813";"30263612";"10479314";;! Cement Kiln Changes: Future emissions are based on permit 1 maximum allowable emission rates.  Wet kiln will be reconstructed to a preheater/precalciner. Ash Grove will use good combustion practices as BACT for VOC (0.138 lb/ton clinker, 12-month rolling period) for the kiln system.: Ash Grove
"48139";;5.75;"71432";;;"4852711";"31648813";"30263612";"10479314";;! Cement Kiln Changes: Future emissions are based on permit 1 maximum allowable emission rates.  Wet kiln will be reconstructed to a preheater/precalciner. Ash Grove will use good combustion practices as BACT for VOC (0.138 lb/ton clinker, 12-month rolling period) for the kiln system.: Ash Grove
"48139";;5.75;"75070";;;"4852711";"31648813";"30263612";"10479314";;! Cement Kiln Changes: Future emissions are based on permit 1 maximum allowable emission rates.  Wet kiln will be reconstructed to a preheater/precalciner. Ash Grove will use good combustion practices as BACT for VOC (0.138 lb/ton clinker, 12-month rolling period) for the kiln system.: Ash Grove
"48139";;4.22;"CO";;;"4852711";"31648813";"30263612";"10479314";;! Cement Kiln Changes: Future emissions are based on permit 1 maximum allowable emission rates.  Wet kiln will be reconstructed to a preheater/precalciner. Ash Grove will use good combustion practices as BACT for CO (1.23 lb/ton clinker, 30-day rolling average) for the kiln system.: Ash Grove
"48139";;6.55;"NH3";;;"4852711";"31648813";"30263612";"10479314";;!  : Future emissions are based on permit 1 maximum allowable emission rates.  Wet kiln will be reconstructed to a preheater/precalciner. An alternative case specific specification (pursuant to 30 TAC 117.3125) for an ammonia emission limit of 35 ppm for the kilns was approved under a permit alterat
"48139";;1.72;"NOX";;;"4852711";"31648813";"30263612";"10479314";;! Cement Kiln Changes: Future emissions are based on permit 1 maximum allowable emission rates.  Wet kiln will be reconstructed to a preheater/precalciner.  NSPS Subpart F limits emissions of NOx for new and reconstructed kilns to less than 1.5 lb/ton clinker, based on a 30-day rolling average.  Ash
"48139";;3.95;"PM10-PRI";;;"4852711";"31648813";"30263612";"10479314";;! Cement Kiln Changes: Ash Grove
"48139";;5.17;"PM25-PRI";;;"4852711";"31648813";"30263612";"10479314";;! Cement Kiln Changes: Ash Grove
"48139";;0.12;"SO2";;;"4852711";"31648813";"30263612";"10479314";;! Cement Kiln Changes: Future emissions are based on permit 1 maximum allowable emission rates. Wet kiln will be reconstructed to a preheater/precalciner kilns.  NSPS Subpart F limits emissions of SO2 for new and reconstructed kilns to less than 0.4 lb/ton clinker, based on a 30-day rolling average,
"48139";;5.75;"VOC";;;"4852711";"31648813";"30263612";"10479314";;! Cement Kiln Changes: Future emissions are based on permit 1 maximum allowable emission rates.  Wet kiln will be reconstructed to a preheater/precalciner. Ash Grove will use good combustion practices as BACT for VOC (0.138 lb/ton clinker, 12-month rolling period) for the kiln system.: Ash Grove
"51670";;3.9756;"NOX";;;"5769011";"20375813";"19638912";"76698514";;! Honeywell International Inc - Hopewell
"51670";;1.4218;"NOX";;;"5769011";"20379913";"19636712";"76696814";;! Honeywell International Inc - Hopewell
"51670";;1.8061;"NOX";;;"5769011";"20380213";"19634612";"76696714";;! Honeywell International Inc - Hopewell
"51670";;1.5011;"NOX";;;"5769011";"20384513";"19635212";"76698414";;! Honeywell International Inc - Hopewell
"51820";;10.3332;"NOX";;;"4958111";"30858913";"29524612";"1836514";;! Invista  - Waynesboro
"51820";;164.0631;"SO2";;;"4958111";"30858913";"29524612";"1836514";;! Invista  - Waynesboro
/END/
