# GSPRO_COMBO for 2023el, stationary sources
#
# PFCs (mode EVP) use 100% profile 8870E
# BTP (no mode) use three profiles according to the splits below, which do not vary by county
# OTAQ previously sent BTP splits for 2017 and 2025, which we interpolated to 2023
#
# POL,FIPS,PERIOD,NPROF,PROF1,FRAC1,PROF2,FRAC2,PROF3,FRAC3,SUMFRAC
#EXPORT_DATE=Wed Oct 16 12:32:09 EDT 2019
#EXPORT_VERSION_NAME=Initial Version
#EXPORT_VERSION_NUMBER=0
"EVP__NONHAPVOC";00000;0;3;8870E;1.0;8871E;0;8934E;0;1
"EVP__VOC";00000;0;3;8870;1.0;8871;0;8934;0;1
"NONHAPVOC";00000;0;3;8870;0.859908737;8871;0.111706428;8934;0.02838475;1
"VOC";00000;0;3;8870;0.859908737;8871;0.111706428;8934;0.02838475;1
