> IM Programs for NJ
> Corrected by EPA June 2005. Valid for 2000 through 2004 calendar years.

> Exhaust I/M program 1
* First I/M program
I/M PROGRAM        : 1 1974 2050 2 TRC IDLE
I/M MODEL YEARS    : 1 1941 1980
I/M VEHICLES       : 1 22222 22222222 2
I/M STRINGENCY     : 1 30.0
I/M COMPLIANCE     : 1 98.0
I/M WAIVER RATES   : 1 0.0 0.0

> Exhaust I/M program 2
* Second I/M program
I/M PROGRAM        : 2 1974 2050 2 TRC ASM 5015 PHASE-IN
I/M MODEL YEARS    : 2 1981 2050
I/M VEHICLES       : 2 22222 11111111 1
I/M STRINGENCY     : 2 30.0
I/M COMPLIANCE     : 2 98.0
I/M WAIVER RATES   : 2 0.0 0.4

> Exhaust I/M program 3
* Third I/M program
I/M PROGRAM        : 3 1974 2050 2 TRC IDLE
I/M MODEL YEARS    : 3 1981 2050
I/M VEHICLES       : 3 11111 22222222 2
I/M STRINGENCY     : 3 30.0
I/M COMPLIANCE     : 3 98.0
I/M WAIVER RATES   : 3 0.0 0.0

> Evaporative I/M program 4
* Fourth I/M program
I/M PROGRAM        : 4 1998 2050 2 TRC GC
I/M MODEL YEARS    : 4 1970 2050
I/M VEHICLES       : 4 22222 22222222 2
I/M COMPLIANCE     : 4 98.0
I/M WAIVER RATES   : 4 0.0 0.0

I/M Effectiveness  :  0.946  0.9383  0.854