> I/M program inputs for 2002 calendar year 
> IM240 Exhaust I/M program for Light Duty vehicles <=10,0000 lb GVWR
*     I/M Effectiveness Set to 0.91/0.93/0.75 for HC/CO/NOx to Reflect MA31 effectiveness as per DEP report July 2003 
*     I/M Grace Period Set to 5 (i.e. exempt 5 newest model years) to Reflect Exemption and LEP 
*     *** Cutpoints file set for 2002 calendar model run
> Corrected by EPA June 2005. Valid for for 2000 through 2002 calendar years.

I/M PROGRAM        : 1 1984 2050 2 TRC IM240
I/M CUTPOINTS      : 1 25000102.imc
I/M MODEL YEARS    : 1 1984 2050
I/M VEHICLES       : 1 22222 21111111 1
I/M STRINGENCY     : 1 20.0
I/M COMPLIANCE     : 1 96.0
I/M WAIVER RATES   : 1 0.0 1.0
I/M GRACE PERIOD   : 1  5

> Two-Speed Idle Exhaust I/M program for Heavy Duty vehicles >10,000 lb GVWR
*     I/M Grace Period Set to 5 (i.e. exempt 5 newest model years) to Reflect Exemption and LEP
I/M PROGRAM        : 2 2000 2050 2 TRC 2500/IDLE
I/M MODEL YEARS    : 2 1984 2050
I/M VEHICLES       : 2 11111 12222222 2
I/M STRINGENCY     : 2 20.0
I/M COMPLIANCE     : 2 96.0
I/M WAIVER RATES   : 2 0.0 1.0
I/M GRACE PERIOD   : 2  5

> Gas Cap Evap I/M program for all vehicles
*     I/M Grace Period Set to 5 (i.e. exempt 5 newest model years) to Reflect Exemption and LEP
I/M PROGRAM        : 3 2000 2050 2 TRC GC
I/M MODEL YEARS    : 3 1984 2050
I/M VEHICLES       : 3 22222 22222222 2
I/M STRINGENCY     : 3 20.0
I/M COMPLIANCE     : 3 96.0
I/M WAIVER RATES   : 3 0.0 1.0
I/M GRACE PERIOD   : 3  5

I/M EFFECTIVENESS  : 0.91 0.93 0.75



