> IM Programs for NJ
* Added ASM5015 beginning 2000, OBD beginning 2005
* New programs include Evap GC
> Adapted from 3400102.imp submitted by NJ for the 2002 NEI
> Corrected by EPA June 2005. Valid for 1998 and 1999 calendar years.

> Exhaust I/M program 1
* Original Idle program.
I/M PROGRAM        : 1 1975 2050 1 T/O IDLE
I/M MODEL YEARS    : 1 1968 2050
I/M VEHICLES       : 1 22222 22222222 2
I/M STRINGENCY     : 1 30.0
I/M COMPLIANCE     : 1 98.0
I/M WAIVER RATES   : 1 0.0 0.4

> Evaporative I/M program 2
* beginning in calendar year 1998.
I/M PROGRAM        : 2 1998 2050 2 TRC GC
I/M MODEL YEARS    : 2 1970 2050
I/M VEHICLES       : 2 22222 22222222 2
I/M COMPLIANCE     : 2 98.0
I/M WAIVER RATES   : 2 0.0 0.0

I/M Effectiveness  :  0.946  0.9383  0.854
