> IM Programs for Utah, County 11.
> Adapted from 2005 NEI I/M file, 
> Extended I/M program end date from 2005 to 2050.
> Adapted by EPA Jan 2008.

I/M PROGRAM        : 1 1984 2050 1 T/O 2500/IDLE
I/M MODEL YEARS    : 1 1968 1995
I/M VEHICLES       : 1 22222 22222222 2
I/M STRINGENCY     : 1 22.6
I/M COMPLIANCE     : 1 96.0
I/M WAIVER RATES   : 1 1.0 1.0
I/M EFFECTIVENESS  : 1.00 1.00 1.00
*First I/M pgm: Cal Years 1984-2050, Test-only,2500/IDLE.
*LDVs of MY 1996-on undergo OBD I/M and EVAP OBD in place of two-speed idle.
*Credit for Technician Training and Certification program begins in 1998.

*Second I/M pgm: Cal Years 1984-2050, Test-only, OBD I/M
I/M PROGRAM        : 2 1984 2050 1 T/O OBD I/M
I/M MODEL YEARS    : 2 1996 2050
I/M VEHICLES       : 2 22222 22222222 2
I/M STRINGENCY     : 2 22.6
I/M COMPLIANCE     : 2 96.0
I/M WAIVER RATES   : 2 1.0 1.0
I/M EFFECTIVENESS  : 1.00 1.00 1.00
*OBD starts in 1997 in Da Co.

*Third I/M pgm: Cal Years 1984-2050, Test-only, EVAP OBD
I/M PROGRAM        : 3 1984 2050 1 T/O EVAP OBD
I/M MODEL YEARS    : 3 1996 2050
I/M VEHICLES       : 3 22222 11111111 1
*I/M STRINGENCY     : 3 22.6
I/M COMPLIANCE     : 3 96.0
I/M WAIVER RATES   : 3 1.0 1.0
I/M EFFECTIVENESS  : 1.00 1.00 1.00
*Do not use I/M STRINGENCY command for evap tests. 
*The User's Guide states that EVAP OBD cannot be applied to HDVs of MY 2006 or earlier. 

*Fourth I/M pgm: Cal Year 2050, Test-only, gas cap pressure test
I/M PROGRAM        : 4 1984 2050 1 T/O GC
I/M MODEL YEARS    : 4 1968 1995
I/M VEHICLES       : 4 22222 22222222 2
*I/M STRINGENCY     : 4 22.6
I/M COMPLIANCE     : 4 96.0
I/M WAIVER RATES   : 4 1.0 1.0
I/M EFFECTIVENESS  : 1.00 1.00 1.00
*EVAP OBD and GAS CAP PRESURE TEST CANNOT BE APPLIED TO A SINGLE PARTICULAR VEHICLE.
*LDVs of model year 1995 and older undergo gas cap pressure test instead of OBD I/M and
*EVAP OBD.  
*All gasoline vehicles of MY 1968 - 1995 undergo GC, including HDGVs, according to Mike Eggington (4-21-06).
*Do not use I/M STRINGENCY command for evap tests. 


