> IM Programs for Utah, County 35 (Salt Lake County).
> Adapted from 2005 NEI I/M file, 
> Extended I/M program end date from 2005 to 2050.
> Adapted by EPA Jan 2008.

I/M PROGRAM        : 1 1984 2050 1 T/O ASM 2525/5015 PHASE-IN 
I/M MODEL YEARS    : 1 1968 1995 
I/M VEHICLES       : 1 22222 11111111 1
I/M STRINGENCY     : 1 22.0
I/M COMPLIANCE     : 1 96.0
I/M WAIVER RATES   : 1 1.0 1.0
I/M EFFECTIVENESS  : 1.00 1.00 1.00
*First I/M pgm: Cal Yrs 1984-2050, Test-only, Two-speed Idle. 
*Effectiveness of test-only pgm is 100%.
*Add credit for Technician Training and Certification (TTC) beginning in 1998.
*OBD startup is deferred until Jan. 2003.
*LDVs of MY older than 1996 undergo ASM. 

*Second I/M pgm: Cal Years 1984-2050, Test-only, 2500/IDLE
I/M PROGRAM        : 2 1984 2050 1 T/O 2500/IDLE
I/M MODEL YEARS    : 2 1968 1995
I/M VEHICLES       : 2 11111 22222222 2
I/M STRINGENCY     : 2 22.0
I/M COMPLIANCE     : 2 96.0
I/M WAIVER RATES   : 2 1.0 1.0
I/M EFFECTIVENESS  : 1.00 1.00 1.00
*HDVs undergo two-speed idle instead of ASM 2525/5015.
*HDVs of MY 1996 - on undergo OBD starting Jan. 2003.  

*Third I/M pgm: Cal Years 1984-2050, Test-only, OBD I/M
I/M PROGRAM        : 3 1984 2050 1 T/O OBD I/M
I/M MODEL YEARS    : 3 1996 2050
I/M VEHICLES       : 3 22222 22222222 2
I/M STRINGENCY     : 3 22.0
I/M COMPLIANCE     : 3 96.0
I/M WAIVER RATES   : 3 1.0 1.0
I/M EFFECTIVENESS  : 1.00 1.00 1.00
*OBD starts in 2003 in SL Co.

*Fourth I/M pgm: Cal Years 1984-2050, Test-only, EVAP OBD & GC
I/M PROGRAM        : 4 1984 2050 1 T/O EVAP OBD & GC
I/M MODEL YEARS    : 4 1998 2050
I/M VEHICLES       : 4 22222 11111111 1
I/M COMPLIANCE     : 4 96.0
I/M WAIVER RATES   : 4 1.0 1.0
*Change MYs to 1998 - 2050 per Richard Valentine; evap does nothing for MY 96-97 per Rick McKeague.
*Also, MUST model EVAP OBD & GC in this single block; cannot model EVAP OBD and GC
*in separate blocks if both test procedures apply to any specific MY.  This is the case even in
*the newest (Sept 2003) version of M6. 
*Latest version of M6 does not allow EVAP OBD to be applied to HDVs of MY 2006 and earlier.  
*I/M EFFECTIVENESS AND I/M STRINGENCY COMMANDS ARE NOT TO BE APPLIED TO EVAP PROGRAMS (SUCH AS EVAP OBD AND GC). 
*See User's Guide, pp. 140 and 148. 

*Fifth I/M pgm: Cal Years 1984 - 2050, Test-only, gas cap pressure test
I/M PROGRAM        : 5 1984 2050 1 T/O GC
I/M MODEL YEARS    : 5 1968 2050
I/M VEHICLES       : 5 11111 22222222 2
I/M STRINGENCY     : 5 22.0
I/M COMPLIANCE     : 5 96.0
I/M WAIVER RATES   : 5 1.0 1.0
I/M EFFECTIVENESS  : 1.00 1.00 1.00
*HDVs of MY 1968-2050 undergo gas cap pressure test because EVAP OBD cannot be applied to
*HDVs of MY older than 2007.

*Sixth I/M pgm: Cal Years 1984-2050, Test-only, gas cap pressure test
I/M PROGRAM        : 6 1984 2050 1 T/O GC
I/M MODEL YEARS    : 6 1968 1997
I/M VEHICLES       : 6 22222 11111111 1
I/M COMPLIANCE     : 6 96.0
I/M WAIVER RATES   : 6 1.0 1.0
*Cannot model the same vehicle under GC and EVAP OBD (as two separate blocks). 
*However, LDVs of MY 1968-1997 undergo GC, and LDVs of MY 1998-on undergo EVAP OBD and GC. 
