# M. Strum  June 20, 2007 fixed typo in mass fraction for STANI profile for NICKEL to NICKEL_F - affects reports but not model-ready emissions
# M Strum changes made 8May2007:  add onroad Beryllium profiles
#EXPORT_DATE=Fri Apr 04 12:31:55 EDT 2025
#EXPORT_VERSION_NAME=add Minnesota
#EXPORT_VERSION_NUMBER=2
#REV_HISTORY v1(08/26/2014)  Allan Beidler.   added arsenic  for 2011v2
#REV_HISTORY v2(12/05/2017)  Christine Allen.   added Minnesota-supplied profiles (85% coarse) to be applied to one point source in Minnesota  for 2014 NATA v2 via PM_Coarse to Fine_Mn_comments.xlsx
#REV_HISTORY v2(12/05/2017)  Christine Allen.   removed Minnesota-specific lead profile  Minnesota did not provide a new split for lead, only the other metals
MNBE;"BERYLLIUM";"BERYLLIUM_F";0.15;1.0;0.15
MNBE;"BERYLLIUM";"BERYLLIUM_C";0.85;1.0;0.85
MNCD;"CADMIUM";"CADMIUM_C";0.85;1.0;0.85
MNCD;"CADMIUM";"CADMIUM_F";0.15;1.0;0.15
MNMN;"MANGANESE";"MANGANESE_C";0.85;1.0;0.85
MNMN;"MANGANESE";"MANGANESE_F";0.15;1.0;0.15
MNNI;"NICKEL";"NICKEL_F";0.15;1.0;0.15
MNNI;"NICKEL";"NICKEL_C";0.85;1.0;0.85
MNRS;"ARSENIC";"ARSENIC_C";0.85;1.0;0.85
MNRS;"ARSENIC";"ARSENIC_F";0.15;1.0;0.15
NOARS;"ARSENIC";"ARSENIC_C";0.17;1.0;0.17
NOARS;"ARSENIC";"ARSENIC_F";0.83;1.0;0.83
NONBE;"BERYLLIUM";"BERYLLIUM_F";0.39;1.0;0.39
NONBE;"BERYLLIUM";"BERYLLIUM_C";0.61;1.0;0.61
NONCD;"CADMIUM";"CADMIUM_F";0.38;1.0;0.38
NONCD;"CADMIUM";"CADMIUM_C";0.62;1.0;0.62
NONMN;"MANGANESE";"MANGANESE_F";0.67;1.0;0.67
NONMN;"MANGANESE";"MANGANESE_C";0.33;1.0;0.33
NONNI;"NICKEL";"NICKEL_F";0.49;1.0;0.49
NONNI;"NICKEL";"NICKEL_C";0.51;1.0;0.51
NONPB;"LEAD";"LEAD_F";0.88;1.0;0.88
NONPB;"LEAD";"LEAD_C";0.12;1.0;0.12
ONBE;"BERYLLIUM";"BERYLLIUM_C";0.61;1.0;0.61! placeholder for onroad beryllium
ONBE;"BERYLLIUM";"BERYLLIUM_F";0.39;1.0;0.39! placeholder for onroad beryllium
ONCD;"CADMIUM";"CADMIUM_C";0.62;1.0;0.62
ONCD;"CADMIUM";"CADMIUM_F";0.38;1.0;0.38
ONMN;"MANGANESE";"MANGANESE_F";0.64;1.0;0.64
ONMN;"MANGANESE";"MANGANESE_C";0.36;1.0;0.36
ONNI;"NICKEL";"NICKEL_F";0.83;1.0;0.83
ONNI;"NICKEL";"NICKEL_C";0.17;1.0;0.17
ONPB;"LEAD";"LEAD_F";0.76;1.0;0.76
ONPB;"LEAD";"LEAD_C";0.24;1.0;0.24
STABE;"BERYLLIUM";"BERYLLIUM_F";0.68;1.0;0.68
STABE;"BERYLLIUM";"BERYLLIUM_C";0.32;1.0;0.32
STACD;"CADMIUM";"CADMIUM_C";0.24;1.0;0.24
STACD;"CADMIUM";"CADMIUM_F";0.76;1.0;0.76
STAMN;"MANGANESE";"MANGANESE_C";0.33;1.0;0.33
STAMN;"MANGANESE";"MANGANESE_F";0.67;1.0;0.67
STANI;"NICKEL";"NICKEL_F";0.59;1.0;0.59
STANI;"NICKEL";"NICKEL_C";0.41;1.0;0.41
STAPB;"LEAD";"LEAD_C";0.26;1.0;0.26
STAPB;"LEAD";"LEAD_F";0.74;1.0;0.74
STARS;"ARSENIC";"ARSENIC_C";0.41;1.0;0.41
STARS;"ARSENIC";"ARSENIC_F";0.59;1.0;0.59
