# LOC = data/preproc/atms_beamwidth.dat
# WMO Satellite ID
224
# Version identifier
1
# Sampling distance (deg)
1.11
# Number of channels to modify
16 
# Channel, beam width, new width, cutoff, nxaverage, nyaverage, QC dist
# Note: to use FFT technique, set new width and cutoff as required and set 
# nxaverage and nyaverage to 0. To use simple averaging set new width to 0.0
# and use nxaverage and nyaverage (e.g. 3 3 for 3x3 averaging).
# QC Dist gives number of points around missing value to flag as missing.
 1 5.2 3.33 0.4 0 0 11
 2 5.2 3.33 0.4 0 0 11
 3 2.2 3.33 0.0 0 0  5
 4 2.2 3.33 0.0 0 0  5
 5 2.2 3.33 0.0 0 0  5 
 6 2.2 3.33 0.0 0 0  5 
 7 2.2 3.33 0.0 0 0  5 
 8 2.2 3.33 0.0 0 0  5 
 9 2.2 3.33 0.0 0 0  5 
10 2.2 3.33 0.0 0 0  5 
11 2.2 3.33 0.0 0 0  5 
12 2.2 3.33 0.0 0 0  5 
13 2.2 3.33 0.0 0 0  5 
14 2.2 3.33 0.0 0 0  5 
15 2.2 3.33 0.0 0 0  5 
16 2.2 3.33 0.0 0 0  5 
