# NLCD 2001 Land Cover Alaska, 3 x 3 Degree: NLCD2001_LC_N57W138

Metadata also available as

# Metadata:

- Identification_Information
- Data_Quality_Information
- Spatial_Data_Organization_Information
- Spatial_Reference_Information
- Entity_and_Attribute_Information
- Distribution_Information
- Metadata_Reference_Information

Identification_Information:
  Citation:
    Citation_Information:
      Originator: U.S. Geological Survey
      Publication_Date: 20150115
      Title: NLCD 2001 Land Cover Alaska, 3 x 3 Degree: NLCD2001_LC_N57W138
      Edition: 1.0
      Geospatial_Data_Presentation_Form: remote-sensing image
      Series_Information:
        Series_Name: None
        Issue_Identification: None
      Publication_Information:
        Publication_Place: Sioux Falls, SD
        Publisher: U.S. Geological Survey
      Other_Citation_Details:
        References: (1) Jin, S., Yang, L., Danielson, P., Homer, C., Fry, J., and Xian, G. 2013. A comprehensive change detection method for updating the National Land Cover Database to circa 2011. Remote Sensing of Environment, 132: 159 175. (2) Xian, G., Homer, C., Dewitz, J., Fry, J., Hossain, N., and Wickham, J., 2011. The change of impervious surface area between 2001 and 2006 in the conterminous United States. Photogrammetric Engineering and Remote Sensing, Vol. 77(8): 758-762. (3) Coulston, J. W., Moisen, G. G., Wilson, B. T., Finco, M. V., Cohen, W. B., and Brewer, C. K. 2012. Modeling percent tree canopy cover: a pilot study. Photogrammetric Engineering & Remote Sensing 78(7): 715-727. The USGS acknowledges the support of USGS and contractor NLCD 2011 Land Cover Mapping Teams in development of data for this map.
      Online_Linkage:
        <http://gisdata.usgs.gov/tdds/downloadfile.php?TYPE=nlcd2001_lc_3x3&ORIG=META&FNAME=NLCD2001_LC_N57W138.zip>
      Online_Linkage:
        <http://tdds.cr.usgs.gov/metadata/nlcd/2001/landcover/3x3/NLCD2001_LC_N57W138.htm>
      Online_Linkage: <http://nationalmap.gov/viewer.html>
  Description:
    Abstract:
      The National Land Cover Database 2001 land cover layer was produced through a cooperative project conducted by the Multi-Resolution Land Characteristics (MRLC) Consortium. The MRLC Consortium is a partnership of federal agencies (www.mrlc.gov), consisting of the U.S. Geological Survey (USGS), the National Oceanic and Atmospheric Administration (NOAA), the U.S. Environmental Protection Agency (EPA), the U.S. Department of Agriculture - Forest Service (USDA-FS), the National Park Service (NPS), the U.S. Fish and Wildlife Service (FWS), the Bureau of Land Management (BLM) and the USDA Natural Resources Conservation Service (NRCS). One of the primary goals of the project is to generate a current, consistent, seamless, and accurate National Land cover Database (NLCD) circa 2001 for the United States at medium spatial resolution. For a detailed definition and discussion on MRLC and the NLCD 2001 products, refer to Homer et al. (2004) and <http://www.mrlc.gov/mrlc2k.asp>. The NLCD 2001 was created by partitioning the U.S. into mapping zones. A total of 66 mapping zones within the conterminous U.S., with an additional 13 in Alaska, were delineated based on ecoregion and geographical characteristics, edge matching features and the size requirement of Landsat mosaics. Questions about the NLCD mapping zones can be directed to the NLCD 2001 land cover mapping team at USGS EROS, Sioux Falls, SD (605) 594-6151 or mrlc@usgs.gov.
    Purpose:
      The goal of this project is to provide the Nation with complete, current and consistent public domain information on its land use and land cover.
    Supplemental_Information:
      Corner Coordinates (projection meters) Upper Left Corner: -2232345(X), 2380125(Y) Lower Right Corner: 1494735(X), 344805(Y)
  Time_Period_of_Content:
    Time_Period_Information:
      Range_of_Dates/Times:
        Beginning_Date: 20000512
        Ending_Date: 20030810
    Currentness_Reference: ground condition
  Status:
    Progress: In work
    Maintenance_and_Update_Frequency: As needed
  Spatial_Domain:
    Bounding_Coordinates:
      West_Bounding_Coordinate: -141
      East_Bounding_Coordinate: -138
      North_Bounding_Coordinate: 60
      South_Bounding_Coordinate: 57
  Keywords:
    Theme:
      Theme_Keyword_Thesaurus: NGDA Portfolio Themes
      Theme_Keyword: NGDA
      Theme_Keyword: National Geospatial Data Asset
      Theme_Keyword: Land Use Land Cover Theme
    Theme:
      Theme_Keyword_Thesaurus: None
      Theme_Keyword: Land Cover
      Theme_Keyword: GIS
      Theme_Keyword: U.S. Geological Survey
      Theme_Keyword: USGS
      Theme_Keyword: digital spatial data
    Theme:
      Theme_Keyword_Thesaurus: ISO 19115 Topic Category
      Theme_Keyword: imageryBaseMapsEarthCover
      Theme_Keyword: 010
    Place:
      Place_Keyword_Thesaurus:
        U.S. Department of Commerce, 1995, Countries, dependencies, areas of special sovereignty, and their principal administrative divisions, Federal Information Processing Standard 10-4,): Washington, D.C., National Institute of Standards and Technology
      Place_Keyword: United States
      Place_Keyword: U.S.
      Place_Keyword: US
  Access_Constraints: None
  Use_Constraints: None
  Point_of_Contact:
    Contact_Information:
      Contact_Organization_Primary:
        Contact_Organization: U.S. Geological Survey
      Contact_Position: Customer Services Representative
      Contact_Address:
        Address_Type: mailing and physical
        Address: USGS EROS
        Address: 47914 252nd Street
        City: Sioux Falls
        State_or_Province: SD
        Postal_Code: 57198-0001
        Country: USA
      Contact_Voice_Telephone: 605/594-6151
      Contact_TDD/TTY_Telephone: 605/594-6933
      Contact_Facsimile_Telephone: 605/594-6589
      Contact_Electronic_Mail_Address: custserv@usgs.gov
      Hours_of_Service: 0800 - 1600 CT, M - F (-6h CST/-5h CDT GMT)
      Contact_Instructions:
        The USGS point of contact is for questions relating to the data display and download from this web site. For questions regarding data content and quality, refer to: <http://www.mrlc.gov/mrlc2k.asp> or email: mrlc@usgs.gov
  Browse_Graphic:
    Browse_Graphic_File_Name:
      <http://tdds.cr.usgs.gov/browse/nlcd/2001/landcover/3x3/NLCD2001_LC_N57W138.jpg>
    Browse_Graphic_File_Description: Tiled NLCD Browse Image
    Browse_Graphic_File_Type: JPEG
  Data_Set_Credit: U.S. Geological Survey
  Security_Information:
    Security_Classification_System: None
    Security_Classification: Unclassified
    Security_Handling_Description: N/A
  Native_Data_Set_Environment:
    Microsoft Windows 7 Version 6.1 (Build 7601: Service Pack 1); ESRI ArcCatalog 9.3.1.4000 (Service Pack 2)

Data_Quality_Information:
  Attribute_Accuracy:
    Attribute_Accuracy_Report: A formal accuracy assessment has not been conducted.
    Quantitative_Attribute_Accuracy_Assessment:
      Attribute_Accuracy_Value: Unknown
      Attribute_Accuracy_Explanation:
        This document and the described land cover map are considered "provisional" until a formal accuracy assessment is completed. The U.S. Geological Survey can make no guarantee as to the accuracy or completeness of this information, and it is provided with the understanding that it is not guaranteed to be correct or complete. Conclusions drawn from this information are the responsibility of the user.
  Logical_Consistency_Report:
    The NLCD 2001 final seamless products for Alaska include: 1) NLCD 2001 Land Cover; 2) NLCD 2001 Percent Developed Imperviousness; 3) NLCD 2001 Tree Canopy Cover (produced by USDA-FS).
  Completeness_Report:
    This NLCD product of Alaska Land Cover layer is the version dated January 15, 2015.
  Positional_Accuracy:
    Horizontal_Positional_Accuracy:
      Horizontal_Positional_Accuracy_Report: N/A
    Vertical_Positional_Accuracy:
      Vertical_Positional_Accuracy_Report: N/A
  Lineage:
    Process_Step:
      Process_Description:
        The 2001 land cover classification was achieved by use of a classification and decision tree method (DT) using a combination of Landsat imagery and ancillary data. The specific DT program employed is called See5, which implements a gain ratio criterion in tree development and pruning (Quinlan, 1993). See5 also implemented several advanced features that can aid and improve land cover classification, including boosting and cross-validation. Boosting is a technique for improving classification accuracy, while cross-validation can provide certain level of estimation regarding the land cover classification quality. To conduct the land cover classification using DT, a large quantity of training data is required. Training data were collected from several combined sources including National Wetlands Inventory (NWI), Alaska Burned Area Emergency Response (BAER), Bureau of Land Management (BLM), Ducks Unlimited (DU), field collected data, and a variety of local data sources. Note that the training data were used to map all land cover classes except for four classes in urban and sub-urban areas (developed open space, low intensity developed, medium intensity developed, high intensity developed). All urban and suburban land cover classes for Alaska were mapped through either a sub-pixel quantification of impervious surfaces using a regression tree modeling method, or through a series of manual classifications that may include roads, towns, and pipeline GIS data gathered for Alaska. Quality assessment of all land cover classes was limited to available high-resolution imagery, previous classifications, and any field collected ground truth. Following the development of the best classification through decision tree modeling, additional steps were required to complete the final land cover product. The four classes in urban and suburban areas were determined by a calibration with known impervious areas in Alaska mapping zone 8, which includes the Anchorage area, a crosswalk of the manually interpreted areas, and a cursory impervious estimate for each mapping zone. From the interpreted developed product, developed areas were grouped into the following four categories: (1) developed open space (imperviousness approximately < 20%), (2) low-intensity developed (imperviousness approximately from 20 - 49%), (3) medium intensity developed (imperviousness approximately from 50 -79%), and (4) high-intensity developed (imperviousness approximately > 79%). Alaska land cover mapping also provided one additional challenge in that some areas of high relief in Alaska are in shadow at the time of nominal Landsat imagery collection. These shadowed areas were classified with the best available methods. However, a land cover containing shadowed areas that were classified will be available upon special request. Other classes of forest and non-forest were combined with the urban classes to complete the land cover product. Finally visual inspection of the classification was made with areas/pixels that were wrongly classified delineated first as an "area of interest" (AOI), subsequently then limited manual editing was done to eliminate the classification error within the AOI. The completed single pixel product was then generalized to a 1 acre (approximately 5 ETM+ 30 m pixel patch) minimum mapping unit product using a "smart eliminate" algorithm. This aggregation program subsumes pixels from the single pixel level to a 5-pixel patch using a queens algorithm at doubling intervals. The algorithm consults a weighting matrix to guide merging of cover types by similarity, resulting in a product that preserves land cover logic as much as possible. Ancillary data used for the land cover prediction - Data Type of DEM composed of 1 band of Continuous Variable Type. Data Type of Slope composed of 1 band of Continuous Variable Type. Data Type of Aspect composed of 1 band of Categorical Variable Type. Data type of Position Index composed of 1 band of Continuous Variable Type. Alaska GPS roads Alaska Pipeline data Alaska Airports layer Alaska Cities layer
      Source_Used_Citation_Abbreviation: Landsat ETM, USDA, FIA, DEM, USGS/EROS
      Process_Date: Unknown
      Source_Produced_Citation_Abbreviation: USGS NLCD
      Process_Contact:
        Contact_Information:
          Contact_Organization_Primary:
            Contact_Organization: U.S. Geological Survey
          Contact_Position: Customer Services Representative
          Contact_Address:
            Address_Type: mailing and physical
            Address: USGS EROS
            Address: 47914 252nd Street
            City: Sioux Falls
            State_or_Province: SD
            Postal_Code: 57198-0001
            Country: USA
          Contact_Voice_Telephone: 605/594-6151
          Contact_TDD/TTY_Telephone: 605/594-6933
          Contact_Facsimile_Telephone: 605/594-6589
          Contact_Electronic_Mail_Address: custserv@usgs.gov
          Hours_of_Service: 0800 - 1600 CT, M - F (-6h CST/-5h CDT GMT)
    Process_Step:
      Process_Description:
        A custom method was developed to update Alaska NLCD from 2001 to 2011. The method was designed to capitalize on available ancillary data and to capture the main land change drivers including: - Fire disturbance and succession, - Forest clearing and harvesting, - Glacier and snow/ice changes, and - Urban change. We began imagery selection by focusing on odd-numbered Landsat paths. We selected as many leaf-on, cloud-free (or few clouds), same-date images in a path as possible, and mosaicked those to create larger mapping units. Final mapping units were composed of one to four Landsat images. For the Aleutians and other islands, cloud-free images were virtually nonexistent, so those areas were not mapped using image processing and models. Instead, they were visually checked for change from the 2001 land cover map using any available Landsat images and Google Earth. For the mainland area of Alaska we created 44 mapping units and used 22 additional Landsat scenes for the visual inspections of the islands. Once mapping units were identified, the base images were cloud-masked. Reference scenes from different dates were used in a model to fill in the masked areas of the base scenes. Once the base scenes were cloud-filled, they were mosaicked to form each full mapping unit. Tasseled cap, normalized burn ratio (NBR), normalized difference vegetation index (NDVI) and normalized difference water index (NDWI) images were calculated for each mapping unit. Ancillary data included: - Digital elevation model (DEM) and derivatives (slope and aspect), - Fire and forest thinning polygons obtained from the state of Alaska, Landfire, and the Monitoring Trends in Burn Severity (MTBS) project, - Moderate Resolution Imaging Spectroradiometer (MODIS) snow/ice raster data, and - 2001 NLCD. Change detection and classification models used NLCD 2001 and ancillary data to predict land cover classes for changed areas. An example of the logic is as follows: If (NLCD 2001 is forest & wildfire occurred less than 4 years ago & dNBR is high & NBR 2011 is low), then it is likely the new land cover type is herbaceous in 2011. The general modeling process was as follows: 1. Biomass increase was calculated from spectral and DEM derivatives, plus 2001 land cover. 2. Biomass increase was added to the disturbance data, yielding a disturbance template. 3. The disturbance template plus the spectral derivatives (NBR, NDVI) were compared to the 2001 land cover to model updated vegetation change areas. 4. The updated vegetation change areas were inserted into the 2001 land cover to create training data for a classification and regression tree (CART) model. 5. A CART classification was used to detect unmapped disturbances and change. 6. The vegetation classification was refined to detect and correct for areas of shadow and succession after forest fires, clearing or thinning. 7. Snow/ice change was detected using an algorithm based on NDWI for 2001 and 2011 plus topography (correction for shadows) and MODIS snow/ice data, which yielded snow/ice change areas. 8. Water change was detected using a Landsat-based water change detection algorithm, refined by land cover and topography data (shadow areas) to detect changes. 9. The vegetation, snow/ice, and water change areas were combined to update the overall classification and to derive a set of change pixels. 10. Change pixels in urban/developed areas were created by modeling change in major cities. Manual editing was used to add developed change for small towns and other features. After all mapping units were processed, the change pixels were mosaicked and checked for consistency and quality. Manual edits were used to clean up areas that were incorrectly classified. Snow, ice, and water extents were mapped directly from Landsat imagery. As a result, the extent of snow, ice, and water reflects the year and season when the imagery was recorded. Differences in snow, ice, and water extent between 2001 and 2011 may not reflect perennial changes in their extent, but simply reflect seasonal change between the two time periods.
      Process_Date: Unknown

Spatial_Data_Organization_Information:
  Direct_Spatial_Reference_Method: Raster
  Raster_Object_Information:
    Raster_Object_Type: Pixel
    Row_Count: 12166
    Column_Count: 8094
    Vertical_Count: 1

Spatial_Reference_Information:
  Horizontal_Coordinate_System_Definition:
    Planar:
      Map_Projection:
        Map_Projection_Name: Albers Conical Equal Area
        Albers_Conical_Equal_Area:
          Standard_Parallel: 55.000000
          Standard_Parallel: 65.000000
          Longitude_of_Central_Meridian: -154.000000
          Latitude_of_Projection_Origin: 50.000000
          False_Easting: 0.000000
          False_Northing: 0.000000
      Planar_Coordinate_Information:
        Planar_Coordinate_Encoding_Method: row and column
        Coordinate_Representation:
          Abscissa_Resolution: 30.000000
          Ordinate_Resolution: 30.000000
        Planar_Distance_Units: meters
    Geodetic_Model:
      Horizontal_Datum_Name: World Geodetic System 1984
      Ellipsoid_Name: World Geodetic System 1984
      Semi-major_Axis: 6378137.0
      Denominator_of_Flattening_Ratio: 298.2572235

Entity_and_Attribute_Information:
  Detailed_Description:
    Entity_Type:
      Entity_Type_Label: Layer_1
      Entity_Type_Definition: NLCD Land Cover Layer
      Entity_Type_Definition_Source: National Land Cover Database
    Attribute:
      Attribute_Label: ObjectID
      Attribute_Definition: Internal feature number
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain:
          Sequential unique whole numbers that are automatically generated.
    Attribute:
      Attribute_Label: Count
      Attribute_Definition:
        A nominal integer value that designates the number of pixels that have each value in the file; histogram column in ERDAS Imagine raster attributes table
      Attribute_Definition_Source: NLCD
      Attribute_Domain_Values:
        Unrepresentable_Domain: Integer
    Attribute:
      Attribute_Label: Value
      Attribute_Definition:
        Land Cover Class Code Value. Class definitions marked with an asterisk (*) are Coastal NLCD Classes only.
      Attribute_Definition_Source: NLCD
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: 0
          Enumerated_Domain_Value_Definition: Background / No Data
          Enumerated_Domain_Value_Definition_Source: NLCD land cover class descriptions
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: 1
          Enumerated_Domain_Value_Definition: No data value, Alaska zones only
          Enumerated_Domain_Value_Definition_Source: NLCD land cover class descriptions
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: 11
          Enumerated_Domain_Value_Definition:
            Open Water - All areas of open water, generally with less than 25% cover or vegetation or soil
          Enumerated_Domain_Value_Definition_Source: NLCD land cover class descriptions
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: 12
          Enumerated_Domain_Value_Definition:
            Perennial Ice/Snow - All areas characterized by a perennial cover of ice and/or snow, generally greater than 25% of total cover.
          Enumerated_Domain_Value_Definition_Source: NLCD land cover class descriptions
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: 21
          Enumerated_Domain_Value_Definition:
            Developed, Open Space - Includes areas with a mixture of some constructed materials, but mostly vegetation in the form of lawn grasses. Impervious surfaces account for less than 20 percent of total cover. These areas most commonly include large-lot single-family housing units, parks, golf courses, and vegetation planted in developed settings for recreation, erosion control, or aesthetic purposes
          Enumerated_Domain_Value_Definition_Source: NLCD land cover class descriptions
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: 22
          Enumerated_Domain_Value_Definition:
            Developed, Low Intensity -Includes areas with a mixture of constructed materials and vegetation. Impervious surfaces account for 20-49 percent of total cover. These areas most commonly include single-family housing units.
          Enumerated_Domain_Value_Definition_Source: NLCD land cover class descriptions
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: 23
          Enumerated_Domain_Value_Definition:
            Developed, Medium Intensity - Includes areas with a mixture of constructed materials and vegetation. Impervious surfaces account for 50-79 percent of the total cover. These areas most commonly include single-family housing units.
          Enumerated_Domain_Value_Definition_Source: NLCD land cover class descriptions
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: 24
          Enumerated_Domain_Value_Definition:
            Developed, High Intensity - Includes highly developed areas where people reside or work in high numbers. Examples include apartment complexes, row houses and commercial/industrial. Impervious surfaces account for 80 to 100 percent of the total cover.
          Enumerated_Domain_Value_Definition_Source: NLCD land cover class descriptions
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: 31
          Enumerated_Domain_Value_Definition:
            Barren Land (Rock/Sand/Clay) - Barren areas of bedrock, desert pavement, scarps, talus, slides, volcanic material, glacial debris, sand dunes, strip mines, gravel pits and other accumulations of earthen material. Generally, vegetation accounts for less than 15% of total cover.
          Enumerated_Domain_Value_Definition_Source: NLCD land cover class descriptions
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: 41
          Enumerated_Domain_Value_Definition:
            Deciduous Forest - Areas dominated by trees generally greater than 5 meters tall, and greater than 20% of total vegetation cover. More than 75 percent of the tree species shed foliage simultaneously in response to seasonal change.
          Enumerated_Domain_Value_Definition_Source: NLCD land cover class descriptions
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: 42
          Enumerated_Domain_Value_Definition:
            Evergreen Forest - Areas dominated by trees generally greater than 5 meters tall, and greater than 20% of total vegetation cover. More than 75 percent of the tree species maintain their leaves all year. Canopy is never without green foliage.
          Enumerated_Domain_Value_Definition_Source: NLCD land cover class descriptions
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: 43
          Enumerated_Domain_Value_Definition:
            Mixed Forest - Areas dominated by trees generally greater than 5 meters tall, and greater than 20% of total vegetation cover. Neither deciduous nor evergreen species are greater than 75 percent of total tree cover.
          Enumerated_Domain_Value_Definition_Source: NLCD land cover class descriptions
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: 51
          Enumerated_Domain_Value_Definition:
            Dwarf Scrub - Alaska only areas dominated by shrubs less than 20 centimeters tall with shrub canopy typically greater than 20% of total vegetation. This type is often co-associated with grasses, sedges, herbs, and non-vascular vegetation tundra and may be periodically or seasonally wet and/or saturated with wate. This type commonly occurs in alpine or tundra areas and may contain permafrost.
          Enumerated_Domain_Value_Definition_Source: NLCD land cover class descriptions
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: 52
          Enumerated_Domain_Value_Definition:
            Shrub/Scrub - Areas dominated by shrubs less than 5 meters tall with shrub canopy typically greater than 20% of total vegetation. This class includes true shrubs, young trees in an early successional stage or trees stunted from environmental conditions.
          Enumerated_Domain_Value_Definition_Source: NLCD land cover class descriptions
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: 71
          Enumerated_Domain_Value_Definition:
            Grassland/Herbaceous - Areas dominated by grammanoid or herbaceous vegetation, generally greater than 80% of total vegetation. These areas are not subject to intensive management such as tilling, but can be utilized for grazing.
          Enumerated_Domain_Value_Definition_Source: NLCD land cover class descriptions
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: 72
          Enumerated_Domain_Value_Definition:
            Sedge/Herbaceous - Alaska only areas dominated by sedges and forbs, generally greater than 80% of total vegetation. This type can occur with significant other grasses or other grass like plants, and includes sedge tundra, and sedge tussock tundra.
          Enumerated_Domain_Value_Definition_Source: NLCD land cover class descriptions
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: 73
          Enumerated_Domain_Value_Definition:
            Lichens - Alaska only areas dominated by fruticose or foliose lichens generally greater than 80% of total vegetation.
          Enumerated_Domain_Value_Definition_Source: NLCD Legend Land Cover Class Descriptions
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: 74
          Enumerated_Domain_Value_Definition:
            Moss- Alaska only areas dominated by mosses generally greater than 80% of total vegetation.
          Enumerated_Domain_Value_Definition_Source: NLCD land cover class descriptions
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: 81
          Enumerated_Domain_Value_Definition:
            Pasture/Hay - Areas of grasses, legumes, or grass-legume mixtures planted for livestock grazing or the production of seed or hay crops, typically on a perennial cycle. Pasture/hay vegetation accounts for greater than 20 percent of total vegetation.
          Enumerated_Domain_Value_Definition_Source: NLCD land cover class descriptions
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: 82
          Enumerated_Domain_Value_Definition:
            Cultivated Crops - Areas used for the production of annual crops, such as corn, soybeans, vegetables, tobacco, and cotton, and also perennial woody crops such as orchards and vineyards. Crop vegetation accounts for greater than 20 percent of total vegetation. This class also includes all land being actively tilled.
          Enumerated_Domain_Value_Definition_Source: NLCD land cover class descriptions
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: 90
          Enumerated_Domain_Value_Definition:
            Woody Wetlands - Areas where forest or shrub land vegetation accounts for greater than 20 percent of vegetative cover and the soil or substrate is persistently saturated with or covered with water.
          Enumerated_Domain_Value_Definition_Source: NLCD land cover class descriptions
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: 95
          Enumerated_Domain_Value_Definition:
            Emergent Herbaceous Wetlands - Areas where perennial herbaceous vegetation accounts for greater than 80 percent of vegetative cover and the soil or substrate is persistently saturated with or covered with water.
          Enumerated_Domain_Value_Definition_Source: NLCD land cover class descriptions
    Attribute:
      Attribute_Label: Red
      Attribute_Definition:
        Numeric code for Red color in RGB slice format for image display purposes. The value is arbitrarily assigned by the display software package, unless defined by user.
      Attribute_Definition_Source: NLCD
      Attribute_Domain_Values:
        Range_Domain:
          Range_Domain_Minimum: 0
          Range_Domain_Maximum: 100
          Attribute_Units_of_Measure: CSS Color Value Percentage
          Attribute_Measurement_Resolution: 0.1
    Attribute:
      Attribute_Label: Green
      Attribute_Definition:
        Numeric code for Green color in RGB slice format for image display purposes. The value is arbitrarily assigned by the display software package, unless defined by user.
      Attribute_Definition_Source: NLCD
      Attribute_Domain_Values:
        Range_Domain:
          Range_Domain_Minimum: 0
          Range_Domain_Maximum: 100
          Attribute_Units_of_Measure: CSS Color Value Percentage
          Attribute_Measurement_Resolution: 0.1
    Attribute:
      Attribute_Label: Blue
      Attribute_Definition:
        Numeric code for Blue color in RGB slice format for image display purposes. The value is arbitrarily assigned by the display software package, unless defined by user.
      Attribute_Definition_Source: NLCD
      Attribute_Domain_Values:
        Range_Domain:
          Range_Domain_Minimum: 0
          Range_Domain_Maximum: 100
          Attribute_Units_of_Measure: CSS Color Value Percentage
          Attribute_Measurement_Resolution: 0.1
    Attribute:
      Attribute_Label: Opacity
      Attribute_Definition:
        A measure of how opaque, or solid, a color is displayed in a layer.
      Attribute_Definition_Source: NLCD
      Attribute_Domain_Values:
        Range_Domain:
          Range_Domain_Minimum: 0
          Range_Domain_Maximum: 100
          Attribute_Units_of_Measure: Percentage
          Attribute_Measurement_Resolution: 0.1
  Overview_Description:
    Entity_and_Attribute_Overview:
      Attributes defined by USGS and ESRI. Class Red Green Blue 0 0.000000000 0.000000000 0.000000000 1 0.000000000 1.000000000 0.000000000 11 0.325490196 0.462745098 0.662745098 12 0.854901961 0.913725490 1.000000000 21 0.913725490 0.819607843 0.815686275 22 0.890196078 0.615686275 0.545098039 23 0.976470588 0.000000000 0.000000000 24 0.705882353 0.000000000 0.000000000 31 0.741176471 0.725490196 0.670588235 41 0.443137255 0.701960784 0.419607843 42 0.137254902 0.423529412 0.231372549 43 0.752941176 0.827450980 0.607843137 51 0.694117647 0.588235294 0.235294118 52 0.835294118 0.764705882 0.533333333 71 0.925490196 0.925490196 0.796078431 72 0.823529412 0.823529412 0.505882353 74 0.513725490 0.725490196 0.619607843 81 0.901960784 0.882352941 0.282352941 82 0.709803922 0.486274510 0.200000000 90 0.760784314 0.878431373 0.949019608 95 0.486274510 0.674509804 0.772549020
    Entity_and_Attribute_Detail_Citation:
      Attribute accuracy is described, where present, with each attribute defined in the Entity and Attribute Section.

Distribution_Information:
  Distributor:
    Contact_Information:
      Contact_Organization_Primary:
        Contact_Organization: U.S. Geological Survey
      Contact_Position: Customer Service Representative
      Contact_Address:
        Address_Type: mailing and physical
        Address: USGS National Geospatial Program Office
        Address: 12201 Sunrise Valley Drive
        City: Reston
        State_or_Province: VA
        Postal_Code: 20192
        Country: USA
      Contact_Voice_Telephone: 1-888-ASK-USGS (1-888-275-8747)
      Contact_Electronic_Mail_Address: tnm_help@usgs.gov
      Hours_of_Service: Monday through Friday 8:00 AM to 4:00 PM Eastern Time Zone USA
      Contact_Instructions: Please visit <http://www.usgs.gov/ask/> to contact us.
  Resource_Description: Downloadable data
  Distribution_Liability:
    Although these data have been processed successfully on a computer system at the USGS, no warranty expressed or implied is made by the USGS regarding the use of the data on any other system, nor does the act of distribution constitute any such warranty. Data may have been compiled from various outside sources. Spatial information may not meet National Map Accuracy Standards. This information may be updated without notification. The USGS shall not be liable for any activity involving these data, installation, fitness of the data for a particular purpose, its use, or analyses results.
  Standard_Order_Process:
    Digital_Form:
      Digital_Transfer_Information:
        Format_Name: TIFF
        Transfer_Size: 1.811685
      Digital_Transfer_Option:
        Online_Option:
          Computer_Contact_Information:
            Network_Address:
              Network_Resource_Name:
                <http://gisdata.usgs.gov/tdds/downloadfile.php?TYPE=nlcd2001_lc_3x3&ORIG=META&FNAME=NLCD2001_LC_N57W138.zip>
          Access_Instructions:
            The URL <http://nationalmap.gov/viewer.html> provides a map interface that allows for viewing and data downloads within a customer defined area of interest. Zoom tools are available that can be used to investigate areas of interest on the map interface. The download tool allows the customer to capture layers from the map, utilizing The National Map process for downloading. The file can be unzipped and imported into various user software applications.
          Online_Computer_and_Operating_System: Not available for dissemination
    Fees: None
    Ordering_Instructions: Contact Customer Service
    Turnaround: Variable
  Custom_Order_Process: Contact Customer Service Representative
  Technical_Prerequisites:
    ESRI ArcGIS Suite and/or Arc/Info or other compatible software, and supporting operating systems.
  Available_Time_Period:
    Time_Period_Information:
      Range_of_Dates/Times:
        Beginning_Date: 2015
        Ending_Date: Unknown

Metadata_Reference_Information:
  Metadata_Date: 20150115
  Metadata_Contact:
    Contact_Information:
      Contact_Organization_Primary:
        Contact_Organization: U.S. Geological Survey
        Contact_Person: Customer Service Representative
      Contact_Position: Customer Services Representative
      Contact_Address:
        Address_Type: mailing and physical
        Address: USGS EROS
        Address: 47914 252nd Street
        City: Sioux Falls
        State_or_Province: SD
        Postal_Code: 57198-0001
        Country: USA
      Contact_Voice_Telephone: 605/594-6151
      Contact_TDD/TTY_Telephone: 605/594-6933
      Contact_Facsimile_Telephone: 605/594-6589
      Contact_Electronic_Mail_Address: custserv@usgs.gov
      Hours_of_Service: 0800 - 1600 CT, M - F (-6h CST/-5h CDT GMT)
  Metadata_Standard_Name: FGDC Content Standard for Digital Geospatial Metadata
  Metadata_Standard_Version: FGDC-STD-001-1998
  Metadata_Time_Convention: local time
  Metadata_Access_Constraints: None
  Metadata_Use_Constraints: None

Generated by `mp` version 2.9.12 on Fri Mar 27 15:39:41 2015