> IM Programs for UT DAVIS COUNTY
> Adapted from 4901102.imp supplied by UT for the 2002 NEI.
> Corrected by EPA June 2005. Valid for 2002 and later calendar years.

I/M PROGRAM        : 1 1984 2050 1 TRC 2500/IDLE
I/M MODEL YEARS    : 1 1968 1995
I/M VEHICLES       : 1 22222 22222222 2
I/M STRINGENCY     : 1 22.0
I/M COMPLIANCE     : 1 96.0
I/M WAIVER RATES   : 1 1.0 1.0
*I/M EFFECTIVENESS  : 0.50 0.50 0.50
*First I/M pgm: Cal Years 1998-2050, Test-and-repair on 2500/IDLE.
*LDVs of MY 1996-on undergo OBD I/M and EVAP OBD in place of two-speed idle.
*Credit for Technician Training and Certification program begins in 1998.

*Second I/M pgm: Cal Years 1984-2050, Test-only, OBD I/M
I/M PROGRAM        : 2 1984 2050 1 T/O OBD I/M
I/M MODEL YEARS    : 2 1996 2050
I/M VEHICLES       : 2 22222 22222222 2
I/M STRINGENCY     : 2 22.0
I/M COMPLIANCE     : 2 96.0
I/M WAIVER RATES   : 2 1.0 1.0
*OBD starts in 1997 in Da Co.

*Third I/M pgm: Cal Years 1984-2050, Test-only, EVAP OBD
I/M PROGRAM        : 3 1984 2050 1 T/O EVAP OBD
I/M MODEL YEARS    : 3 1996 2050
I/M VEHICLES       : 3 22222 11111111 1
I/M STRINGENCY     : 3 22.0
I/M COMPLIANCE     : 3 96.0
I/M WAIVER RATES   : 3 1.0 1.0

*Fourth I/M pgm: Cal Year 2002, Test-only, gas cap pressure test
I/M PROGRAM        : 4 1984 2050 1 T/O GC
I/M MODEL YEARS    : 4 1968 1995
I/M VEHICLES       : 4 22222 11111111 1
I/M STRINGENCY     : 4 22.0
I/M COMPLIANCE     : 4 96.0
I/M WAIVER RATES   : 4 1.0 1.0
*EVAP OBD and GAS CAP PRESURE TEST CANNOT BE APPLIED TO A SINGLE PARTICULAR VEHICLE.
*LDVs of model year 1995 and older undergo gas cap pressure test instead of OBD I/M and
*EVAP OBD.  

*Fifth I/M pgm: Test-only, gas cap pressure test
I/M PROGRAM        : 5 1984 2050 1 T/O GC
I/M MODEL YEARS    : 5 1968 2006
I/M VEHICLES       : 5 11111 22222222 2
I/M STRINGENCY     : 5 22.0
I/M COMPLIANCE     : 5 96.0
I/M WAIVER RATES   : 5 1.0 1.0
*EVAP OBD CANNOT BE APPLIED TO AN HDV of model year 2006 or older. 

*Seventh I/M pgm: Test-only, Evap OBD for HDV 2007 and newer
I/M PROGRAM        : 7 1984 2050 1 T/O GC
I/M MODEL YEARS    : 7 2007 2050
I/M VEHICLES       : 7 11111 22222222 2
I/M STRINGENCY     : 7 22.0
I/M COMPLIANCE     : 7 96.0
I/M WAIVER RATES   : 7 1.0 1.0
*EVAP OBD CAN ONLY BE APPLIED TO AN HDV of model year 2007 and NEWER.

I/M EFFECTIVENESS  : 1.00 1.00 1.00
 



