> IM Programs for UT Utah County
I/M PROGRAM        : 1 1986 2050 1 T/O 2500/IDLE
I/M MODEL YEARS    : 1 1968 1995 
I/M VEHICLES       : 1 22222 22222222 2
I/M STRINGENCY     : 1 14.0
I/M COMPLIANCE     : 1 96.0
I/M WAIVER RATES   : 1 0.1 0.1
I/M EXEMPTION AGE  : 1 25
I/M EFFECTIVENESS  : 1.00 1.00 1.00
*First I/M pgm: Cal Yrs 1986-2050, Test-only, Two-speed Idle. 
*Effectiveness of test-only pgm is 100% (beginning in 1996).
*Add credit for Technician Training and Certification (TTC) beginning in 1998.

I/M PROGRAM        : 2 1986 2050 1 T/O OBD I/M
I/M MODEL YEARS    : 2 1996 2050
I/M VEHICLES       : 2 22222 22222222 2
I/M STRINGENCY     : 2 14.0
I/M COMPLIANCE     : 2 96.0
I/M WAIVER RATES   : 2 0.1 0.1
I/M EXEMPTION AGE  : 2 25
I/M EFFECTIVENESS  : 1.00 1.00 1.00
*Second I/M pgm: Cal Yrs 1986-2050, Test-only, Two-speed Idle. 
*OBD started in 2001 in Utah County.

*Third I/M pgm: Cal Years 1986-2050, Test-only, EVAP OBD
I/M PROGRAM        : 3 1986 2050 1 T/O EVAP OBD
I/M MODEL YEARS    : 3 1996 2050
I/M VEHICLES       : 3 22222 11111111 1
I/M STRINGENCY     : 3 14.0
I/M COMPLIANCE     : 3 96.0
I/M WAIVER RATES   : 3 0.1 0.1
I/M EXEMPTION AGE  : 3 25
I/M EFFECTIVENESS  : 1.00 1.00 1.00
*Check waiver rates in TSD.
*This block is for EVAP OBD on LDVs only.  Model year coverage and start years DIFFER
*between LDVs and HDVs. 

*Fourth I/M pgm: Cal Years 1986-2050, Test-only, EVAP OBD
I/M PROGRAM        : 4 1986 2050 1 T/O EVAP OBD
I/M MODEL YEARS    : 4 2007 2050
I/M VEHICLES       : 4 11111 22222222 2
I/M STRINGENCY     : 4 14.0
I/M COMPLIANCE     : 4 96.0
I/M WAIVER RATES   : 4 0.1 0.1
I/M EFFECTIVENESS  : 1.00 1.00 1.00
*Jan 2002 version of M6 does not allow EVAP OBD to be applied to HDVs of MY 2006 and earlier.
*Program execution should skip this block because there are no 2007 MY HDVs in the fleet
*in calendar year 2002.  Thus block may be kept active or starred out. 


