* cutpoints instructed to be used ONLY for IM240. Hence that command is not
* used in this IDLE IM program
* IDLE IM program stopped with model year 1995 
* because OBD starts in 2002 and applies for 
* vehicle model years 1996 and newer. So this will avoid double-counting of 
* IM effects. 

* THESE PROGRAMS APPLY FOR ANALYSIS YEARS 2002 through 2015
> Corrected by EPA June 2005. Valid for 1984 and later calendar years.

* IDLE IM program for model years till 1995.

I/M PROGRAM        : 1 1984 2050 1 T/O IDLE
I/M MODEL YEARS    : 1 1974 1995
I/M VEHICLES       : 1 22222 22222222 1
I/M STRINGENCY     : 1 17.0
I/M COMPLIANCE     : 1 84.0
I/M WAIVER RATES   : 1 1.0 1.0
I/M EXEMPTION AGE  : 1 25
I/M GRACE PERIOD   : 1 1

* Exhaust OBD IM program for LDGV, LDGTs and HDGVs model yrs 2002-2050

I/M PROGRAM        : 2 2002 2050 1 T/O OBD I/M
I/M MODEL YEARS    : 2 1996 2050
I/M VEHICLES       : 2 22222 22222222 1
I/M STRINGENCY     : 2 17.0
I/M COMPLIANCE     : 2 84.0
I/M WAIVER RATES   : 2 1.0 1.0

* EVAP OBD and GC IM program for model years till 2006 for LDGV and LDGTs. 

I/M PROGRAM        : 3 2002 2050 1 T/O EVAP OBD & GC
I/M MODEL YEARS    : 3 1996 2006
I/M VEHICLES       : 3 22222 11111111 1
I/M STRINGENCY     : 3 17.0
I/M COMPLIANCE     : 3 84.0
I/M WAIVER RATES   : 3 1.0 1.0

* GC IM program for model years till 2006 for HDGVs. Had to be separated 
* from the IM program#3, because EVAP OBD cannot be applied to HDGVs 
* before model year 2007.

I/M PROGRAM        : 4 2002 2050 1 T/O GC
I/M MODEL YEARS    : 4 1996 2006
I/M VEHICLES       : 4 11111 22222222 1
I/M STRINGENCY     : 4 17.0
I/M COMPLIANCE     : 4 84.0
I/M WAIVER RATES   : 4 1.0 1.0

* EVAP OBD and GC IM program for model years 2007-2050 for LDGV, LDGTs,HDGVs.

I/M PROGRAM        : 5 2002 2050 1 T/O EVAP OBD & GC
I/M MODEL YEARS    : 5 2007 2050
I/M VEHICLES       : 5 22222 22222222 1
I/M STRINGENCY     : 5 17.0
I/M COMPLIANCE     : 5 84.0
I/M WAIVER RATES   : 5 1.0 1.0