VMT BY HOUR
*
*  Fraction of all vehicle miles traveled by hour of the day.     
*  First hour is 6 a.m.  These data are for the Chicago NAA for 
*   2007, derived from Dean Englund's TM output in MF12.xls, as 
*   calculated on page "DE vmtbyhr"
*
*  This file is HVMTCH7.SL, representing SL's estimate of VMT by hour.  
*   SL's estimates are based on Dean's data, but assume VMT in multi-hour 
*   modeling periods is distributed as the default is distributed across 
*   the hours in question.  
*
      0.0443  0.0851  0.0755  0.0577  0.0541  0.0583
      0.0609  0.0572  0.0659  0.0701  0.0818  0.0769
      0.0576  0.0447  0.0219  0.0188  0.0138  0.0102
      0.0077  0.0061  0.0058  0.0057  0.0070  0.0132
*
*  Following , for information, are Dean's estimates of VMT by hour.  
*  Dean assumes that VMT in CATS multi-hour modeling periods is 
*   evenly distributed across the hours in questions (e.g., see hrs
*   2 and 3, both of which are 0.0803, or hours 15-24, which are all 
*   0.0110).  See HVMTCH07.DE for more info about DE's numbers.
*
*      0.0443  0.0803  0.0803  0.0577  0.0576  0.0576
*      0.0576  0.0576  0.0680  0.0680  0.0793  0.0793
*      0.0511  0.0511  0.0110  0.0110  0.0110  0.0110
*      0.0110  0.0110  0.0110  0.0110  0.0110  0.0110
*
*  These following are the default values from HVMT.DEF
*   supplied for comparison.
*      0.0569  0.0740  0.0655  0.0555  0.0540  0.0582
*      0.0608  0.0571  0.0598  0.0636  0.0777  0.0730
*      0.0501  0.0389  0.0308  0.0264  0.0194  0.0144
*      0.0108  0.0086  0.0081  0.0080  0.0098  0.0186
*