> Exhaust and Evaporative I/M setups for Harris County
> Adapted from 4821002.imp provided by TX for the 2002 NEI.
> Corrected by EPA June 2005. Valid for 1997 through 2001 calendar years.

> Exhaust I/M: 2500/IDLE (all HDG)
I/M PROGRAM        : 1 1997 2050 1 TRC 2500/IDLE
I/M MODEL YEARS    : 1 1978 2050
I/M VEHICLES       : 1 11111 22222222 2
I/M STRINGENCY     : 1 20
I/M COMPLIANCE     : 1 96
I/M WAIVER RATES   : 1 3 3
I/M GRACE PERIOD   : 1 2

> Exhaust I/M: ASM 2525/5015 PHASE-IN (LDG 95-)
I/M PROGRAM        : 2 1997 2050 1 TRC ASM 2525/5015 PHASE-IN
I/M MODEL YEARS    : 2 1978 2050
I/M VEHICLES       : 2 22222 11111111 1
I/M STRINGENCY     : 2 20
I/M COMPLIANCE     : 2 96
I/M WAIVER RATES   : 2 3 3
I/M GRACE PERIOD   : 2 2

> Evaporative I/M:  GC (all vehicles) 
I/M PROGRAM        : 4 1997 2050 1 TRC GC
I/M MODEL YEARS    : 4 1978 2050
I/M VEHICLES       : 4 22222 22222222 2
I/M COMPLIANCE     : 4 96
I/M WAIVER RATES   : 4 3 3
I/M GRACE PERIOD   : 4 2

I/M EFFECTIVENESS  : 1 1 1
