* ILLINOIS ENHANCED I/M DESCRIPTION Filename: ILLOBDIM.D
*  OBD EXH AND GAS CAP 1996+ BEGINNING IN 2002

* The Illinois I/M is Biennial Test Only (2 T/O) program
*  that applies to LDGVs, LDGTs, and, in slightly different
*  fashion, to HDGVs.  Exhaust & Evaporative OBD is for 
*  MY '96+ vehicles; IM240 and simple Idle tets remain for 
*  pre-'96 LDVs pre-'81 LDVs respectively.
> Corrected by EPA June 2005. Valid for for 2002 and later calendar years.

* -------------------------------------------------
* Program Description for older LDVs' I/M programs
* -------------------------------------------------

* First I/M program--IDLE test for MY 1968+ LDVs
I/M PROGRAM        : 1 1986 2050 2 T/O IDLE
I/M MODEL YEARS    : 1 1968 1980
I/M VEHICLES       : 1 22222 11111111 1
I/M STRINGENCY     : 1 20.0
I/M COMPLIANCE     : 1 95.0
I/M WAIVER RATES   : 1 0.5 2.2     '01 data
I/M GRACE PERIOD   : 1 4
*
* Second I/M program--IM240 for MY 1981 to 1995 LDVs
*  "MYCUTS" set to E: drive 15.xij.03 after new
*   computer shifted M6.2 to Zip Drive on E:.
I/M PROGRAM        : 2 1986 2050 2 T/O IM240
I/M MODEL YEARS    : 2 1981 1995
I/M VEHICLES       : 2 22222 11111111 1
I/M STRINGENCY     : 2 20.0
I/M CUTPOINTS      : 2 17000202.imc
I/M COMPLIANCE     : 2 95.0
I/M WAIVER RATES   : 2 0.5 2.2     '01 data
I/M GRACE PERIOD   : 2 4
*
* Third I/M program Gas Cap Check for MY 1968 to 1995 LDVs
I/M PROGRAM        : 3 1992 2050 2 T/O GC
I/M MODEL YEARS    : 3 1968 1995
I/M VEHICLES       : 3 22222 11111111 1
* I/M STRINGENCY not required in evaporative I/M program input
I/M COMPLIANCE     : 3 95.0
I/M WAIVER RATES   : 3 0.5 2.2     '01 data
I/M GRACE PERIOD   : 3 4

* --------------------------------------------------------
* Program description for LDV Evaporative and Exhaust OBD
* -------------------------------------------------------- 

* Fourth I/M program--EVAP OBD & Gas Cap Check for 1996+ LDV
I/M PROGRAM        : 4 2002 2050 2 T/O EVAP OBD & GC
I/M MODEL YEARS    : 4 1996 2050
I/M VEHICLES       : 4 22222 11111111 1
* I/M STRINGENCY not required in evaporative I/M program input
I/M COMPLIANCE     : 4 95.0
I/M WAIVER RATES   : 4 0.5 2.2     '01 data
I/M GRACE PERIOD   : 4 4

* Fifth I/M program--"Exhaust" OBD for MY 1996+ LDVs
I/M PROGRAM        : 5 2002 2050 2 T/O OBD I/M
I/M MODEL YEARS    : 5 1996 2050
I/M VEHICLES       : 5 22222 11111111 1
I/M STRINGENCY     : 5 20.0
I/M COMPLIANCE     : 5 95.0
I/M WAIVER RATES   : 5 0.5 2.2     '01 data
I/M GRACE PERIOD   : 5 4

* -----------------------------------------------
* Program description for Heavy-Duty Vehicle I/M 
* -----------------------------------------------

* Sixth I/M program--HDV IDLE for MY 1968+ HDVs
I/M PROGRAM        : 6 1986 2050 2 T/O IDLE
I/M MODEL YEARS    : 6 1968 2050
I/M VEHICLES       : 6 11111 22222222 2
I/M STRINGENCY     : 6 20.0
I/M COMPLIANCE     : 6 95.0
I/M WAIVER RATES   : 6 1.2 1.5     '01 data
I/M GRACE PERIOD   : 6 4
*
* Seventh I/M program--Gas Cap Check for MY 1968+ HDVs
I/M PROGRAM        : 7 1992 2050 2 T/O GC
I/M MODEL YEARS    : 7 1968 2050
I/M VEHICLES       : 7 11111 22222222 2
* I/M STRINGENCY not required in evaporative I/M program input
I/M COMPLIANCE     : 7 95.0
I/M WAIVER RATES   : 7 1.2 1.5     '01 data
I/M GRACE PERIOD   : 7 4
*
* ----------------
*
* NOTES:
* This is the standard Illinois I/M input, describing
*  the I/M program with OBD as it exists after early 
*  March 2002.  It is the file to be used for regular
*  M6 I/M runs for 2002 and future years.  
*
* This file was originally ILIM3.D, by Jim Matheny
*  of IEPA/BOA/VIM, supplied to SL by JM 12.iij.02 and
*  verified by SL.  JM's original ILIM3.D has been 
*  slightly revised by the addition of comments such 
*  as this one.  The actual inputs have not been changed,
*  except to:
* (a) Move and renumber "Exhaust OBD", JM's original 
*      Program 7, to Program 5, and renumber JM's 
*      Programs 5 and 6 to Programs 6 and 7.  This
*      was done to put the two OBD programs (exhaust
*      and evaporative) together.  The order of the 
*      programs in the I/M file has no effect, but 
*      they must be numbered sequentially.
* (b) Direct the I/M CUTPOINTS in the Second Program
*      from JM's original c:\M6\RUN\EXAMPLES/MYCUTS.D
*      [sic] to E:\MOBILE62\RUN\EXAMPLES\MYCUTS.D for 
*      use on SL's computer.
* JM verified that this file as shown is correctly
*  describes the I/M program for the 2002 Inventory
*  (Jan '04).
* ----------------
