> IM Programs for UT Weber County
> Adapted from 4905702.imp provided by UT for the 2002 NEI by EPA.
> Valid for calendar years 2002 and later.

I/M PROGRAM        : 1 1992 2050 1 TRC 2500/IDLE
I/M MODEL YEARS    : 1 1968 1995 
I/M VEHICLES       : 1 22222 22222222 2
I/M STRINGENCY     : 1 22.0
I/M COMPLIANCE     : 1 96.0
I/M WAIVER RATES   : 1 3.0 3.0
*I/M EFFECTIVENESS  : 0.50 0.50 0.50
*First I/M pgm: Actual cal yrs 2001-2006, test-and-repair credit at 50%,
*two-speed Idle. 
*I/M pgm original start year is 1992.
*The first program year must be the original I/M program start year, which is 1992.
*Effectiveness of test-and-repair pgm is 50%. 
*TTC is in effect. 

*Second I/M pgm: Actual cal yrs 2001-2006, test-only, OBD I/M
I/M PROGRAM        : 2 1992 2050 1 T/O OBD I/M
I/M MODEL YEARS    : 2 1996 2006
I/M VEHICLES       : 2 22222 22222222 2
I/M STRINGENCY     : 2 22.0
I/M COMPLIANCE     : 2 96.0
I/M WAIVER RATES   : 2 3.0 3.0
*OBD starts in 2001. All OBD programs receive test-only credit at 100%.
*OBD applies to all vehicles. The program ends in 2006 because, starting in 2007, this I/M
*file will be appended to include EVAP OBD on the HDVs.

*Third I/M pgm: Actual cal years 2001-2006, test-only, EVAP OBD
I/M PROGRAM        : 3 1992 2050 1 T/O EVAP OBD
I/M MODEL YEARS    : 3 1996 2006
I/M VEHICLES       : 3 22222 11111111 1
I/M STRINGENCY     : 3 22.0
I/M COMPLIANCE     : 3 96.0
I/M WAIVER RATES   : 3 3.0 3.0
*EVAP OBD cannot be run on HDVs of MY earlier than 2007.

I/M EFFECTIVENESS  : 1.00 1.00 1.00

 
