> IM Programs for Utah, County 49 (Utah County).
> Adapted from 2005 NEI I/M file, 
> Extended I/M program end date from 2005 to 2050.
> Adapted by EPA Jan 2008.

I/M PROGRAM        : 1 1986 2050 1 T/O 2500/IDLE
I/M MODEL YEARS    : 1 1968 1995 
I/M VEHICLES       : 1 22222 22222222 2
I/M STRINGENCY     : 1 32.0
I/M COMPLIANCE     : 1 96.0
I/M WAIVER RATES   : 1 0.1 0.1
I/M EXEMPTION AGE  : 1 25
I/M EFFECTIVENESS  : 1.00 1.00 1.00
*First I/M pgm: Cal Yrs 1986-2050, Test-only, Two-speed Idle. 
*Effectiveness of test-only pgm is 100% (beginning in 1996).
*Add credit for Technician Training and Certification (TTC) beginning in 1998.

*Second I/M pgm: Cal Yrs 1986-2050, Test-only, OBD I/M 
I/M PROGRAM        : 2 1986 2050 1 T/O OBD I/M
I/M MODEL YEARS    : 2 1996 2050
I/M VEHICLES       : 2 22222 22222222 2
I/M STRINGENCY     : 2 32.0
I/M COMPLIANCE     : 2 96.0
I/M WAIVER RATES   : 2 0.1 0.1
I/M EXEMPTION AGE  : 2 25
I/M EFFECTIVENESS  : 1.00 1.00 1.00
*OBD started in 2001 in Utah County.

*Third I/M pgm: Cal Years 1986-2050, Test-only, EVAP OBD
I/M PROGRAM        : 3 1986 2050 1 T/O EVAP OBD
I/M MODEL YEARS    : 3 1996 2050
I/M VEHICLES       : 3 22222 11111111 1
*I/M STRINGENCY     : 3 32.0
I/M COMPLIANCE     : 3 96.0
I/M WAIVER RATES   : 3 0.1 0.1
I/M EXEMPTION AGE  : 3 25
I/M EFFECTIVENESS  : 1.00 1.00 1.00
*Check waiver rates in TSD.
*This block is for EVAP OBD on LDVs only. 
*User's Guide states that EVAP OBD cannot be applied on HDVs of MY older than 2007. 
*Do not use I/M STRINGENCY command for evaporative tests (e.g, EVAP OBD or GC). 




